ANNEX 1
TECHNICAL SPECIFICATIONS OF THE CONTAINER SKIP TRUCK

	Item
	Specifications
	Bidder's Information

	ENGINE
	Number of cylinders: 6 in-line cylinders with turbocharger
	

	
	Minimum power: 155 kW
	

	
	Minimum torque: 750 Nm
	

	
	Fuel system: Direct injection
	

	
	Fuel: Diesel
	

	
	Drive configuration: 4×2 or 6×4
	

	
	Minimum payload capacity: 5,500 kg (4×2) or 8,500 kg (6×4)
	

	
	Cooling system: Water-cooled
	

	TRANSMISSION
	Manual gearbox with a minimum of 6 forward gears and rear differential lock
	

	
	Single-disc clutch, with or without assistance (pneumatic, hydraulic or hydro-pneumatic)
	

	SUSPENSION
	Front: Reinforced semi-elliptic or parabolic suspension, consistent with the declared payload capacity
	

	
	Rear: Bogie (tandem) suspension or equivalent reinforced semi-elliptic suspension
	

	STEERING
	Hydraulic power steering; right-hand drive (RHD)
	

	BRAKES
	Pneumatic braking system with drum or disc friction brakes on both front and rear axles
	

	
	Anti-lock Braking System (ABS) mandatory
	

	TYRES AND WHEELS
	11.00R22.5 tyres (or equivalent size with equal or higher load index), dual rear wheels
	

	SAFETY
	Fire extinguisher
	

	HYDRAULIC SYSTEM
	Hydraulic system for lifting and handling waste containers with a minimum capacity of 6 m³, operated through a Power Take-Off (PTO)
	

	TRAINING
	Training for 4 operators on operation and preventive maintenance of the equipment
	

	AFTER-SALES SERVICE AND WARRANTY
	Official manufacturer's representative with a branch in the province
	

	
	Documentary evidence of the availability of spare parts (e.g. stock list, supply agreement or declaration from the local representative)
	

	
	Minimum one-year manufacturer's warranty from the date of delivery/acceptance, supported by the manufacturer's official warranty certificate
	








ANEXO 1
ESPECIFICAÇÕES TÉCNICA DE CAMIÃO PORTA-CONTENTOR
	Item
	Especificações
	Informações do concorrente

	MOTOR
	Número de Cilindros: 6 cilindros em linha com turbo
	

	
	Potência mínima: 155 kW
	

	
	Torque mínimo: 750 Nm
	

	
	Alimentação: Sistema de injecção
	

	
	Combustível: diesel
	

	
	Tracção: 4x2 ou 6x4
	

	
	Capacidade de Carga mínima: 5.500 kg (tracção 4x2) ou 8.500 kg (tracção 6x4). 
	

	
	Tipo de Refrigeração: água
	

	TRANSMISSÃO
	Caixa: manual, mínimo de 6 velocidades, bloqueio de diferencial traseiro
	

	
	Embraiagem: monodisco, com ou sem assistência (pneumática, hidráulica ou hidro-pneumática)
	

	SUSPENSÃO
	Dianteira: semi-elíptica ou parabólica, reforçada de forma consistente com a capacidade de carga declarada
	

	
	Traseira: tipo bogie (tandem) ou semi-elíptica reforçada equivalente
	

	DIRECÇÃO
	Assistida hidraulicamente; volante posicionado à direita
	

	TRAVÕES
	Sistema de travagem pneumático, com mecanismo de fricção a tambor ou a disco, à frente e atrás
	

	
	Sistema antibloqueio de travões (ABS) obrigatório
	

	PNEUS E RODAS
	11.00R22.5 (ou medida equivalente com índice de carga igual ou superior), rodado duplo no(s) eixo(s) traseiro(s)
	

	SEGURANÇA
	Extintor de incêndio
	

	SISTEMA HIRAÚLICO
	Para remoção e manuseamento de contentor, com capacidade mínima de 6 m³, comandado por tomada de força (PTO)
	

	CAPACITAÇÃO
	Capacitação de 4 pessoas sobre operação e manutenção preventiva do equipamento
	

	ASSISTÊNCIA E GARANTIA
	Representante oficial da marca com filial na província
	

	
	Comprovativo documental de disponibilidade de peças sobresselentes (ex. lista de stock, acordo de fornecimento, ou declaração do representante local)
	

	
	Garantia mínima de 1 ano a partir da entrega/aceitação, com certificado oficial do fabricante
	




