ANNEX 2 
ECHNICAL SPECIFICATIONS OF THE TIPPER TRUCK – LOT 2 
	Item
	Specifications
	Bidder's Information

	ENGINE
	Minimum power: 86 kW at the manufacturer's rated engine speed
	

	
	Minimum torque: 400 Nm at the manufacturer's rated engine speed
	

	
	Engine displacement: 3,760–6,630 cm³
	

	
	Fuel system: Direct injection
	

	
	Fuel: Diesel
	

	
	Drive configuration: 4×2 or 4×4 (4WD)
	

	
	Minimum payload capacity: 4,000 kg with a Gross Vehicle Weight (GVW) not exceeding 12,000 kg
	

	
	Cooling system: Water-cooled
	

	
	Type: Truck with tipper body
	

	TRANSMISSION
	Manual, synchromesh gearbox with a minimum of 6 forward gears
	

	
	Clutch suitable for the transmission type
	

	SUSPENSION
	Front: Reinforced semi-elliptic leaf springs with shock absorbers
	

	
	Rear: Reinforced semi-elliptic leaf springs with shock absorbers
	

	STEERING
	Hydraulic power steering
	

	BRAKES
	Pneumatic braking system
	

	
	Disc and/or drum brakes on both front and rear axles
	

	
	Parking/emergency brake with spring-actuated rear brake system
	

	TYRES AND WHEELS
	Single front tyres and dual rear tyres, with a load index appropriate for the vehicle's Gross Vehicle Weight (GVW)
	

	SAFETY
	Fire extinguisher
	

	HYDRAULIC SYSTEM
	Hydraulic tipping system for lifting the cargo body
	

	BODYWORK
	Reinforced tipper body suitable for the transportation of waste and other materials
	

	TRAINING
	Training for 4 operators on operation and preventive maintenance of the equipment
	

	AFTER-SALES SERVICE AND WARRANTY
	Official manufacturer's representative with a branch in the province
	

	
	Documentary evidence of the availability of spare parts (e.g. stock list, supply agreement or declaration from the local representative)
	

	
	Minimum one-year manufacturer's warranty from the date of delivery/acceptance, supported by the manufacturer's official warranty certificate
	




ANEXO 2 
ESPECIFICAÇÕES TÉCNICAS DA CAMIONETA BASCULANTE – LOTE 2
	Item
	Especificações
	Informações do concorrente

	MOTOR
	Potência: mínimo de 86 kW no regime nominal indicado pelo fabricante
	

	
	Torque: mínimo de 400 Nm no regime nominal do fabricante
	

	
	Cilindrada: 3760 cc – 6630 cc
	

	
	Alimentação: sistema de injecção
	

	
	Combustível: diesel (gasóleo)
	

	
	Tracção: 4x2 ou 4x4 (4WD)
	

	
	Capacidade de carga: mínimo de 4.000 kg com Peso Bruto de Viatura (PBV) não superior a 12.000 kg
	

	
	Tipo de refrigeração: água
	

	
	Tipo: camião com carroçaria basculante
	

	TRANSMISSÃO
	Caixa: manual e sincronizada com mínimo de 6 velocidades
	

	
	Embraiagem: sistema adequado ao tipo de transmissão
	

	SUSPENSÃO
	Dianteira: molas semi-elípticas (de lâmina), com amortecedores
	

	
	Traseira: molas semi-elípticas reforçadas (de lâmina), com amortecedores
	

	DIRECÇÃO
	Assistida, hidráulica
	

	TRAVÕES
	Sistema pneumático
	

	
	Travões de disco e/ou tambor à frente e atrás
	

	
	Travão de estacionamento/emergência com mola traseira
	

	PNEUS
	Pneus: dianteiros de rodado simples e traseiros de rodado duplo, dimensionados com índice de carga adequado ao PBV do veículo
	

	SEGURANÇA
	Extintor de incêndio
	

	SISTEMA HIDRÁULICO
	Sistema basculante hidráulico para elevação da caixa de carga
	

	CARROÇARIA
	Caixa basculante reforçada, adequada para transporte de resíduos e materiais diversos
	

	CAPACITAÇÃO
	Formação de 4 operadores em operação e manutenção preventiva do equipamento
	

	ASSISTÊNCIA E GARANTIA
	Representante oficial da marca com filial na província
	

	
	Evidência por parte do fornecedor de facilidade de aquisição de peças sobresselentes
	

	
	Garantia contra defeitos de fabrico mínima de um ano
	



